Used 24 gauge wire

165 turns with 2 bundle fill (40%)

Unacceptable won’t fit in stator slot